格式: airmon-ng <start|stop|check> <interface> [channel or frequency]

airmon-ng <开始|停止|检查> <接口> [信道或频率]